
	Item
No.
	Item Description
(Refuse Collection vehicle for collection of municipal solid waste, 8 m3 capacity) 4 Units
The vehicle must comply with Machinery Directive 2006/42EG or equivalent and be approved by an accredited EC type-examination body 



	1
	General requirements

	1.1
	New vehicle: The Vehicle to be procured must be new: This is assumed if – no more than 12 month have been elapsed between the production of the Vehicle (Chassic and the body structure) and the transfer of ownership of the Vehicle to GIZ
The vehicles have not been used in road traffic and off-road (outside the production site) and do not exceed a mileage of 1500 km

The manufacturer's specified standard equipment for the vehicle model offered is part of the specification and must therefore be included in the delivery

	1.2
	Number of axles: 2

	1.3
	Gros Vehicle Weight 14 tonnes or above 

	1.4
	It is required that at minimum 4.8 – 6 tonnes of waste can be collected.


	2
	Engine

	[bookmark: _Hlk214254022]2.1
	Fuel type: Diesel engine (Euro 5)  

	2.2
	At least 4 cylinders, direct injection

	2.3
	Engine capacity: 2800 cc- 8000 cc

	2.4
	Engine power (minimum): Not less than 180 hp 

	2.5
	Fuel tank volume (minimum): 90 liters

	2.6
	Turbocharged, 

	3
	Transmission

	3.1
	Automated or Automatic gearbox without clutch pedal.

	3.2
	PTO (Power Take off and RPM (Revolution per Minute) limit (<1200)

	4
	Cabin

	4.1
	Number of seats: 1 driver seat + 1 or 2 passenger seats 2 + 1 preferred 

	4.2
	Central Door looking system

	4.3
	Two keys (Min)

	4.4
	Air conditioning (cooling and heating) Required CFC free 

	4.5
	Cabin specs (Driver plus two crew seating) Audio basic

	5.
	Braking system

	5.1
	Front disc brakes, rear disc or drum brakes (for both)

	5.2
	ABS brake system or ESP (Electronic Stability Program)

	5.3
	Air Brake system 

	5.4
	Engine Brake or Exhaust Brake or equivalent 

	6
	Suspension

	6.1
	Front suspension - coil springs, hydraulic shock absorbers

	6.2
	Rear suspension - coil springs, hydraulic shock absorbers

	7
	Steering system

	7.1
	Front wheels - ordinary, rear wheels – dual

	7.2
	Tires of same size per axle (front axle same size, rear axle same size)

	 7.3
	Power Steering

	8
	Compaction equipment, hydraulic system

	8.1
	Compactor useful volume (approx.): 8 m3

	8.2
	Compaction ratio ≥5:1

	8.3
	Loading hopper capacity (approx.): 1 m3

	8.4
	Hydraulic system for rear loading of Euro type containers - suitable for 120,240,770 and 1,100 liters.


	8.5
	Hydraulic system full automatic control integrated with lifting device and provided with two hydraulic cylinders for lifting and lowering tailgate 

	8.6
	Compaction cycle time: 25 - 35 seconds

	8.7
	Body material: Hardox or equivalent, specify thicknesses.
Body sides , roof and floor should be constructed of high tensile steel sheets (to be specified in details)

	8.8
	Sewage water tank under tailgate with outlet

	8.9
	Automatic + Manual control for compaction functions

	8.10
	Hydraulic safety sensors

	8.11
	Lifting system details: two-stage, 800 kg

	8.12
	Low hydraulic oil level safety sensor

	8.13
	Self lubricating system 

	9
	Electrical system

	9.1
	Electrical system 12–24V, 2 beacon lamps

	9.2
	Orange beacon 

	9.3
	Emergency stop systems /Control box and emergency stop at tailgate

	9.4
	Side marker lights

	
	Possibility of managing the superstructure operations from the cabin using a multifunctional control panel with operation indicators, as well as control of operations from the side of the vehicle with the option of two-handed lowering for safety

	9.5
	The rear camera is connected to the same control panel and transmits the image on a minimum screen size of 7”

	10
	Additional equipment

	10.1
	First aid kit

	10.2
	Extinguisher, minimum 8 kg

	10.3
	Reflective triangle

	10.4
	Warning lamp

	10.5
	Hydraulic jack

	10.6
	Tire inflation pump and hose

	10.7
	Tool set

	10.8
	2 safety wedges

	10.9
	Spare wheel

	10.10
	Foldable anti-skid footboards

	10.11
	Self-lubrication system for compaction device.

	11
	Other requirements

	11.1
	Service book and warranties in Engl. language

	11.2
	Spare parts catalog with diagrams for hydraulic and electrical systems

	11.3
	Color requirement: White body RAL 9010

	11.4
	Necessary spare parts list included

	12
	Warranty and /Sales Service /Delivery:

	12.1
	Accompanying documents: Certificate of origin, design copy including dimensions, materials of construction, standards, etc.

	
	
The model offered has been approved by the manufacturer for use in the country of destination Jordan


	12.2
	
Repair and maintenance services, as well as spare parts, for the vehicle/model offered, are available in Jordan, the country of use.

This includes (in particular):
- Maintenance services of the delivered vehicle/model in accordance with the manufacturer's specifications.  
- Repair services of the delivered vehicle/model in accordance with the manufacturer's specifications
- Provision of OEM spare parts for the delivered vehicle/model

Bidders are required to expressly confirm compliance with this requirement in their bid (PDF) and provide the addresses of the service centers and distribution partner(s) in Jordan






 
