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Annex: A preliminary outline of the envisaged Boiler Code

CHAPTER I GENERAL REQUIREMENTS, APPLICATION OF STANDARD CONDITIONS AND EXCEPTIONS THERETO

STANDARD REQUIREMENTS

PROCEDURE FOR RECOGNITION OF COMPETENT AUTHORITY, INSPECTING AUTHORITY, WELL-KNOWN MATERIAL TESTING LABORATORY, WELL-KNOWN STEEL MAKER, WELL-KNOWN FOUNDRY/FORGE, WELL-KNOWN TUBE/PIPE MAKER AND WELL-KNOWN REMANENT LIFE ASSESSMENT ORGANISATION

CHAPTER II 

MATERIALS OF CONSTRUCTION STEEL PLATES, RIVETS, SECTION AND BARS IN CARBON STEEL

WROUGHT IRON STAY AND RIVET BARS

COPPER PLATES, STAY AND RIVET BARS

COLD DRAWN SEAMLESS CARBON STEEL BOILER, SUPERHEATER AND HEAT EX-CHANGER TUBES FOR DESIGN METAL TEMPERATURES NOT EXCEEDING 454°C (850°F)

SEAMLESS CARBON STEEL PIPES FOR HIGH TEMPERATURE SERVICE FOR DESIGN METAL TEMPERATURES NOT EXCEEDING 454°C (850°F)

SEAMLESS FERRITIC AND AUSTENITIC ALLOY STEEL BOILER, SUPERHEATER AND HEAT EXCHANGER TUBES

SEAMLESS FERRITIC PIPES FOR HIGH TEMPERATURE SERVICE

ELECTRIC-RESISTANCE-WELDED STEEL BOILER AND SUPERHEATER TUBES FOR DESIGN METAL TEMPERATURES NOT EXCEEDING 454'C (850'F)

COLD DRAWN-RESISTANCE-WELDED STEEL BOILER AND SUPER-HEATER TUBES FOR DESIGN METAL TEMPERATURE NOT EXC.EEDING 454'C (850'F)

STEEL CASTING

FORGED OR ROLLED PRESSURE PARTS OTHER THAN SEAMLESS DRUMS OR CARBON STEEL

GENERAL GREY IRON CASTINGS (GRADE A)

COVERED ELECTRODES FOR METAL ARC WELDING OR MILD STEEL

FILLER ROADS FOR GAS WELDING OF STEEL

CHAPTER Ill CONSTRUCTION AND WORKMANSHIP 
GENERAL
SHELLS, ANGLE RINGS, BUIT STRAPS, ETC.

END PLATES

FURNACES

STAYS

SCREWED STAYS 

GIRDER STAYS

GUSSET STAYS

BOILER TUBES SUBJECT TO EXTERNAL PRESSURE

STAY TUBES

BOILER AND SUPERHEATER TUBES SUBJECT TO INTERNAL PRESSURE

HEADERS, MUD BOXES, ETC. OF WATER TUBE BOILERS

STAND PIPES, PADS ETC.

MANHOLES, MUDHOLES, ETC.

RIVETING

CHAPTER IV REGULATIONS FOR DETERMINING THE WORKING PRESSURE TO BE ALLOWED ON VARIOUS PARTS OF BOILERS OTHER THAN FUSION WELDED AND SEAMLESS FORGED DRUMS

SHELLS

DISHED END PLATES

FLAT PLATES

STAYS

TUBE PLATES

BOILER AND SUPERHEATER TUBES SUBJECT TO INTERNAL PRESSURE

HEADERS AND SECTION BOXES OF WATER TUBE BOILERS
BOILER TUBES (SMOKE) SUBJECT TO EXTERNAL PRESSURE

FURNACES

SUPPORTS FOR COMBUSTION CHAMBER AND FIREBOX CROWN

PATENT FIREBOX ROOFS OF LOCOTYPE BOILERS

CHAPTER V FUSION WELDED AND SEAMLESS FORGED DRUMS FOR WATER TUBE BOILERS AND SUPERHEATERS

MATERIALS OF CONSTRUCTION

SEAMLESS FORGED DRUMS

TUBES, PIPES IN BOILERS, HEADERS AND STEEL CASTINGS

FUSION WELDED DRUMS

INSPECTION AND TESTING

REGULATION FOR DETERMINING THE WORKING PRESSURE OF WATER TUBE BOILERS WITH FUSION WELDED AND SEAMLESS FORGED DRUMS SHELLS

END PLATES

STANDPIPES AND NOZZLES

CHAPTER VI VALVES, GAUGES AND AUXILIARIES

GENERAL REQUIREMENTS

METHOD OF CONSTRUCTION

SPECIAL REQUIREMENTS SAFETY VALVES

STOP VALVES

BLOW-DOWN COCK OR VALVE AND PIPES

WATER GAUGES

PRESSURE GAUGES

FUSIBLE PLUGS

FEED VALVES

CHAPTER VII BOILER AND SUPERHEATER TUBES, HEADERS & OTHER PARTS TUBES

HEADERS AND SIMILAR PRESSURE PARTS

CHAPTER VIII


STEAM-PIPES AND FITTINGS
MATERIAL
FLANGES
STEAM-PIPE FITTINGS AND CONNECTIONS
STEEL BUTT WELDING FITTING
STEAM RECEIVERS, SEPARATORS, CATCH WATERS, ACCUMULATORS AND SIMILAR VESSELS

CHAPTER IX 
REGULATIONS FOR THE REGISTRATION OF BOILERS AND INSPECTION OF BOILERS AND STEAM-PIPES

CHAPTERIXA SAFETY OF PERSONS INSIDE BOILERS

CHAPTER X 
ELECTRODE BOILERS 
GENERAL REQUIREMENTS
RIVETED STEEL BOILERS
FUSION WELDED BOILERS
TESTS FOR CLASS I FUSION WELDED SEAMS
SEAMLESS SHELL BOILERS

CHAPTER XI 
STANDARD CONDITION FOR THE DESIGN AND CONSTRUCTION OF ECONOMISERS, FEED PIPES, FEED HEATERS AND OTHER SIMILAR VESSELS ECONOMISERS

CAST IRON, TUBES AND HEADERS

CONSTRUCTION REQUIREMENTS CAST IRON ECONOMISERS

STEEL ECONOMISERS WITH OR WITHOUT CAST IRON SLEEVES ON THE TUBES

JOINT BOLTS AND STUDS

VALVES AND MOUNTINGS

FEED PIPES

REGULATION FOR REGISTRATION AND INSPECTION OF ECONOMISERS AND FEED PIPES

TUBES
CHAPTER XII

SHELL TYPE BOILERS OF WELDED CONSTRUCTION

CHAPTER XIII 

QUALIFICATION TESTS FOR WELDERS ENGAGED IN WELDING OF BOILERS AND STEAM-PIPES UNDER CONSTRUCTION, ERECTION AND FABRICATION AT SITE IN INDIA AND IN REPAIRING BOILERS AND STEAM-PIPES BY WELDING

CHAPTER XIV
SMALL INDUSTRIAL BOILERS
GENERAL
CHAPTER XV
FEED WATER FOR BOILER
FORMS
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